#! /bin/sh
# iproute2 version, default updown script
#
# Copyright (C) 2003-2004 Nigel Meteringham
# Copyright (C) 2003-2004 Tuomo Soini
# Copyright (C) 2002-2004 Michael Richardson
# Copyright (C) 2005-2006 Andreas Steffen <andreas.steffen@strongswan.org>
# 
# This program is free software; you can redistribute it and/or modify it
# under the terms of the GNU General Public License as published by the
# Free Software Foundation; either version 2 of the License, or (at your
# option) any later version.  See <http://www.fsf.org/copyleft/gpl.txt>.
# 
# This program is distributed in the hope that it will be useful, but
# WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
# or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
# for more details.
#
# RCSID $Id: _updown.in,v 1.2 2006/04/17 15:06:29 as Exp $

# CAUTION:  Installing a new version of strongSwan will install a new
# copy of this script, wiping out any custom changes you make.  If
# you need changes, make a copy of this under another name, and customize
# that, and use the (left/right)updown parameters in ipsec.conf to make
# strongSwan use yours instead of this default one.

# things that this script gets (from ipsec_pluto(8) man page)
#
#      PLUTO_VERSION
#              indicates  what  version of this interface is being
#              used.  This document describes version  1.1.   This
#              is upwardly compatible with version 1.0.
#
#       PLUTO_VERB
#              specifies the name of the operation to be performed
#              (prepare-host, prepare-client, up-host, up-client,
#              down-host, or down-client).  If the address family
#              for security gateway to security gateway communica­
#              tions is IPv6, then a suffix of -v6 is added to the
#              verb.
#
#       PLUTO_CONNECTION
#              is the name of the  connection  for  which  we  are
#              routing.
#
#       PLUTO_NEXT_HOP
#              is the next hop to which packets bound for the peer
#              must be sent.
#
#       PLUTO_INTERFACE
#              is the name of the ipsec interface to be used.
#
#       PLUTO_REQID
#              is the requid of the ESP policy
#
#       PLUTO_ME
#              is the IP address of our host.
#
#       PLUTO_MY_ID
#              is the ID of our host.
#
#       PLUTO_MY_CLIENT
#              is the IP address / count of our client subnet.  If
#              the  client  is  just  the  host,  this will be the
#              host's own IP address / max (where max  is  32  for
#              IPv4 and 128 for IPv6).
#
#       PLUTO_MY_CLIENT_NET
#              is the IP address of our client net.  If the client
#              is just the host, this will be the  host's  own  IP
#              address.
#
#       PLUTO_MY_CLIENT_MASK
#              is  the  mask for our client net.  If the client is
#              just the host, this will be 255.255.255.255.
#
#       PLUTO_MY_SOURCEIP
#              if non-empty, then the source address for the route will be
#              set to this IP address.
#
#       PLUTO_MY_PROTOCOL
#              is the IP protocol that will be transported.
#
#       PLUTO_MY_PORT
#              is  the  UDP/TCP  port  to  which  the IPsec SA  is
#              restricted on our side.
#
#       PLUTO_PEER
#              is the IP address of our peer.
#
#       PLUTO_PEER_ID
#              is the ID of our peer.
#
#       PLUTO_PEER_CA
#              is the CA which issued the cert of our peer.
#
#       PLUTO_PEER_CLIENT
#              is the IP address / count of the peer's client sub­
#              net.   If the client is just the peer, this will be
#              the peer's own IP address / max (where  max  is  32
#              for IPv4 and 128 for IPv6).
#
#       PLUTO_PEER_CLIENT_NET
#              is the IP address of the peer's client net.  If the
#              client is just the peer, this will  be  the  peer's
#              own IP address.
#
#       PLUTO_PEER_CLIENT_MASK
#              is  the  mask  for  the  peer's client net.  If the
#              client   is   just   the   peer,   this   will   be
#              255.255.255.255.
#
#       PLUTO_PEER_PROTOCOL
#              is the IP protocol that will be transported.
#
#       PLUTO_PEER_PORT
#              is  the  UDP/TCP  port  to  which  the IPsec SA  is
#              restricted on the peer side.
#

# uncomment to log VPN connections
VPN_LOGGING=1
#
# tag put in front of each log entry:
TAG=vpn
#
# syslog facility and priority used:
FAC_PRIO=local0.notice
#
# to create a special vpn logging file, put the following line into
# the syslog configuration file /etc/syslog.conf:
#
# local0.notice                   -/var/log/vpn
#

# check interface version
case "$PLUTO_VERSION" in
1.[0|1])	# Older Pluto?!?  Play it safe, script may be using new features.
	echo "$0: obsolete interface version \`$PLUTO_VERSION'," >&2
	echo "$0: 	called by obsolete Pluto?" >&2
	exit 2
	;;
1.*)	;;
*)	echo "$0: unknown interface version \`$PLUTO_VERSION'" >&2
	exit 2
	;;
esac

# check parameter(s)
case "$1:$*" in
':')			# no parameters
	;;
iptables:iptables)	# due to (left/right)firewall; for default script only
	;;
custom:*)		# custom parameters (see above CAUTION comment)
	;;
*)	echo "$0: unknown parameters \`$*'" >&2
	exit 2
	;;
esac

# utility functions for route manipulation
# Meddling with this stuff should not be necessary and requires great care.
uproute() {
	doroute add
	ip route flush cache
}
downroute() {
	doroute delete
	ip route flush cache
}

addsource() {
	st=0
	if ! ip -o route get ${PLUTO_MY_SOURCEIP%/*} | grep -q ^local
	then
	    it="ip addr add ${PLUTO_MY_SOURCEIP%/*}/32 dev $PLUTO_INTERFACE"
	    oops="`eval $it 2>&1`"
	    st=$?
	    if test " $oops" = " " -a " $st" != " 0"
	    then
		oops="silent error, exit status $st"
	    fi
	    if test " $oops" != " " -o " $st" != " 0"
	    then
		echo "$0: addsource \`$it' failed ($oops)" >&2
	    fi
	fi
	return $st
}

doroute() {
	st=0
	parms="$PLUTO_PEER_CLIENT"

	parms2=
	if [ -n "$PLUTO_NEXT_HOP" ]
	then
	   parms2="via $PLUTO_NEXT_HOP"
	fi
	parms2="$parms2 dev $PLUTO_INTERFACE"

	if [ -z "$PLUTO_MY_SOURCEIP" ]
	then
	    if [ -f /etc/sysconfig/defaultsource ]
	    then
		. /etc/sysconfig/defaultsource
	    fi

	    if [ -f /etc/conf.d/defaultsource ]
	    then
		. /etc/conf.d/defaultsource
	    fi

	    if [ -n "$DEFAULTSOURCE" ]
	    then
		PLUTO_MY_SOURCEIP=$DEFAULTSOURCE
	    fi
        fi

	parms3=
	if test "$1" = "add" -a -n "$PLUTO_MY_SOURCEIP"
	then
	    addsource
	    parms3="$parms3 src ${PLUTO_MY_SOURCEIP%/*}"
	fi

	case "$PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK" in
	"0.0.0.0/0.0.0.0")
		# opportunistic encryption work around
		# need to provide route that eclipses default, without 
		# replacing it.
		it="ip route $1 0.0.0.0/1 $parms2 $parms3 &&
			ip route $1 128.0.0.0/1 $parms2 $parms3"
		;;
	*)	it="ip route $1 $parms $parms2 $parms3"
		;;
	esac
	oops="`eval $it 2>&1`"
	st=$?
	if test " $oops" = " " -a " $st" != " 0"
	then
	    oops="silent error, exit status $st"
	fi
	if test " $oops" != " " -o " $st" != " 0"
	then
	    echo "$0: doroute \`$it' failed ($oops)" >&2
	fi
	return $st
}
 
# in the presence of KLIPS and ipsecN interfaces do not use IPSEC_POLICY 
if [ `echo "$PLUTO_INTERFACE" | grep "ipsec"` ]
then
	IPSEC_POLICY_IN=""
	IPSEC_POLICY_OUT=""
else
	IPSEC_POLICY="-m policy --pol ipsec --proto esp --reqid $PLUTO_REQID"
	IPSEC_POLICY_IN="$IPSEC_POLICY --dir in"
	IPSEC_POLICY_OUT="$IPSEC_POLICY --dir out"
fi

# are there port numbers?
if [ "$PLUTO_MY_PORT" != 0 ]
then
	S_MY_PORT="--sport $PLUTO_MY_PORT"
	D_MY_PORT="--dport $PLUTO_MY_PORT"
fi
if [ "$PLUTO_PEER_PORT" != 0 ]
then
	S_PEER_PORT="--sport $PLUTO_PEER_PORT"
	D_PEER_PORT="--dport $PLUTO_PEER_PORT"
fi

# the big choice
case "$PLUTO_VERB:$1" in
prepare-host:*|prepare-client:*)
	# delete possibly-existing route (preliminary to adding a route)
	case "$PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK" in
	"0.0.0.0/0.0.0.0")
		# need to provide route that eclipses default, without 
		# replacing it.
		parms1="0.0.0.0/1"
		parms2="128.0.0.0/1"
		it="ip route delete $parms1 2>&1 ; ip route delete $parms2 2>&1"
		oops="`ip route delete $parms1 2>&1 ; ip route delete $parms2 2>&1`"
		;;
	*)
		parms="$PLUTO_PEER_CLIENT"
		it="ip route delete $parms 2>&1"
		oops="`ip route delete $parms 2>&1`"
		;;
	esac
	status="$?"
	if test " $oops" = " " -a " $status" != " 0"
	then
		oops="silent error, exit status $status"
	fi
	case "$oops" in
	*'RTNETLINK answers: No such process'*)	
		# This is what route (currently -- not documented!) gives
		# for "could not find such a route".
		oops=
		status=0
		;;
	esac
	if test " $oops" != " " -o " $status" != " 0"
	then
		echo "$0: \`$it' failed ($oops)" >&2
	fi
	exit $status
	;;
route-host:*|route-client:*)
	# connection to me or my client subnet being routed
	uproute
	;;
unroute-host:*|unroute-client:*)
	# connection to me or my client subnet being unrouted
	downroute
	;;
up-host:)
	# connection to me coming up
	# If you are doing a custom version, firewall commands go here.
	;;
down-host:)
	# connection to me going down
	# If you are doing a custom version, firewall commands go here.
	;;
up-client:)
	# connection to my client subnet coming up
	# If you are doing a custom version, firewall commands go here.
	;;
down-client:)
	# connection to my client subnet going down
	# If you are doing a custom version, firewall commands go here.
	;;
up-host:iptables)
	# connection to me, with (left/right)firewall=yes, coming up
	# This is used only by the default updown script, not by your custom
	# ones, so do not mess with it; see CAUTION comment up at top.
	iptables -I INPUT 1 -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	    -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	    -d $PLUTO_ME $D_MY_PORT $IPSEC_POLICY_IN -j ACCEPT
	iptables -I OUTPUT 1 -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	    -s $PLUTO_ME $S_MY_PORT $IPSEC_POLICY_OUT \
	    -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT -j ACCEPT
	#
	# log IPsec host connection setup
	if [ $VPN_LOGGING ]
	then
	  if [ "$PLUTO_PEER_CLIENT" == "$PLUTO_PEER/32" ]
	  then
	    logger -t $TAG -p $FAC_PRIO \
	      "+ `echo -e $PLUTO_PEER_ID` $PLUTO_PEER -- $PLUTO_ME"
	  else
	    logger -t $TAG -p $FAC_PRIO \
	      "+ `echo -e $PLUTO_PEER_ID` $PLUTO_PEER_CLIENT == $PLUTO_PEER -- $PLUTO_ME"
	  fi
	fi	
	;;
down-host:iptables)
	# connection to me, with (left/right)firewall=yes, going down
	# This is used only by the default updown script, not by your custom
	# ones, so do not mess with it; see CAUTION comment up at top.
	iptables -D INPUT -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	    -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	    -d $PLUTO_ME $D_MY_PORT $IPSEC_POLICY_IN -j ACCEPT
	iptables -D OUTPUT -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	    -s $PLUTO_ME $S_MY_PORT $IPSEC_POLICY_OUT \
	    -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT -j ACCEPT
	#
	# log IPsec host connection teardown
	if [ $VPN_LOGGING ]
	then
	  if [ "$PLUTO_PEER_CLIENT" == "$PLUTO_PEER/32" ]
	  then
	    logger -t $TAG -p $FAC_PRIO -- \
	      "- `echo -e $PLUTO_PEER_ID` $PLUTO_PEER -- $PLUTO_ME"
	  else
	    logger -t $TAG -p $FAC_PRIO -- \
	    "- `echo -e $PLUTO_PEER_ID` $PLUTO_PEER_CLIENT == $PLUTO_PEER -- $PLUTO_ME"
	  fi
	fi
	;;
up-client:iptables)
	# connection to client subnet, with (left/right)firewall=yes, coming up
	# This is used only by the default updown script, not by your custom
	# ones, so do not mess with it; see CAUTION comment up at top.
	if [ "$PLUTO_PEER_CLIENT" != "$PLUTO_MY_SOURCEIP/32" ]
	then
	  iptables -I FORWARD 1 -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	      -s $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $S_MY_PORT \
	      -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT \
	         $IPSEC_POLICY_OUT -j ACCEPT
	  iptables -I FORWARD 1 -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	      -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	      -d $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $D_MY_PORT \
	         $IPSEC_POLICY_IN -j ACCEPT
	fi
	#
	# a virtual IP requires an INPUT and OUTPUT rule on the host
	# or sometimes host access via the internal IP is needed
	if [ -n "$PLUTO_MY_SOURCEIP" -o -n "$PLUTO_HOST_ACCESS" ]
	then
	  iptables -I INPUT 1 -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	      -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	      -d $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $D_MY_PORT \
	         $IPSEC_POLICY_IN -j ACCEPT
	  iptables -I OUTPUT 1 -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	      -s $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $S_MY_PORT \
	      -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT \
	         $IPSEC_POLICY_OUT -j ACCEPT
	fi
	#
	# log IPsec client connection setup
	if [ $VPN_LOGGING ]
	then
	  if [ "$PLUTO_PEER_CLIENT" == "$PLUTO_PEER/32" ]
	  then
	    logger -t $TAG -p $FAC_PRIO \
	      "+ `echo -e $PLUTO_PEER_ID` $PLUTO_PEER -- $PLUTO_ME == $PLUTO_MY_CLIENT"
	  else
	    logger -t $TAG -p $FAC_PRIO \
	      "+ `echo -e $PLUTO_PEER_ID` $PLUTO_PEER_CLIENT == $PLUTO_PEER -- $PLUTO_ME == $PLUTO_MY_CLIENT"
	  fi
	fi
	;;
down-client:iptables)
	# connection to client subnet, with (left/right)firewall=yes, going down
	# This is used only by the default updown script, not by your custom
	# ones, so do not mess with it; see CAUTION comment up at top.
	if [ "$PLUTO_PEER_CLIENT" != "$PLUTO_MY_SOURCEIP/32" ]
	then
	  iptables -D FORWARD -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	      -s $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $S_MY_PORT \
	      -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT \
	         $IPSEC_POLICY_OUT -j ACCEPT
	  iptables -D FORWARD -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	      -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	      -d $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $D_MY_PORT \
	         $IPSEC_POLICY_IN -j ACCEPT
	fi
	#
	# a virtual IP requires an INPUT and OUTPUT rule on the host
	# or sometimes host access via the internal IP is needed
	if [ -n "$PLUTO_MY_SOURCEIP" -o -n "$PLUTO_HOST_ACCESS" ]
	then
	  iptables -D INPUT -i $PLUTO_INTERFACE -p $PLUTO_MY_PROTOCOL \
	      -s $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $S_PEER_PORT \
	      -d $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $D_MY_PORT \
	         $IPSEC_POLICY_IN -j ACCEPT
	  iptables -D OUTPUT -o $PLUTO_INTERFACE -p $PLUTO_PEER_PROTOCOL \
	      -s $PLUTO_MY_CLIENT_NET/$PLUTO_MY_CLIENT_MASK $S_MY_PORT \
	      -d $PLUTO_PEER_CLIENT_NET/$PLUTO_PEER_CLIENT_MASK $D_PEER_PORT \
	         $IPSEC_POLICY_OUT -j ACCEPT
	fi
	#
	# log IPsec client connection teardown
	if [ $VPN_LOGGING ]
	then
	  if [ "$PLUTO_PEER_CLIENT" == "$PLUTO_PEER/32" ]
	  then
	    logger -t $TAG -p $FAC_PRIO -- \
	      "- `echo -e $PLUTO_PEER_ID` $PLUTO_PEER -- $PLUTO_ME == $PLUTO_MY_CLIENT"
	  else
	    logger -t $TAG -p $FAC_PRIO -- \
	      "- `echo -e $PLUTO_PEER_ID` $PLUTO_PEER_CLIENT == $PLUTO_PEER -- $PLUTO_ME == $PLUTO_MY_CLIENT"
	  fi
	fi
	;;
#
# IPv6
#
prepare-host-v6:*|prepare-client-v6:*)
	;;
route-host-v6:*|route-client-v6:*)
	# connection to me or my client subnet being routed
	#uproute_v6
	;;
unroute-host-v6:*|unroute-client-v6:*)
	# connection to me or my client subnet being unrouted
	#downroute_v6
	;;
up-host-v6:*)
	# connection to me coming up
	# If you are doing a custom version, firewall commands go here.
	;;
down-host-v6:*)
	# connection to me going down
	# If you are doing a custom version, firewall commands go here.
	;;
up-client-v6:)
	# connection to my client subnet coming up
	# If you are doing a custom version, firewall commands go here.
	;;
down-client-v6:)
	# connection to my client subnet going down
	# If you are doing a custom version, firewall commands go here.
	;;
*)	echo "$0: unknown verb \`$PLUTO_VERB' or parameter \`$1'" >&2
	exit 1
	;;
esac
